**1.Addition of two 8 bit nos.**

#include<stdio.h>

#include<stdlib.h>

#include<p18f4550.h>

void main(void)

{

int sum;

sum =0;

sum= 0x05+0X02;

TRISD=0;

PORTD=sum;

}